**Score Sheet #1- Tractor Inspection**

Contestant \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

School\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Region\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Participant is dressed appropriately for this CDE and is wearing work boots. (If box is not checked prior to the event starting, then the student may not participate on the driving course)**

**TRACTOR INSPECTION RESPONSE (verbal response to Judges) Faults Points**

Check fuel and oil gauges \_\_\_\_ X 10 \_\_\_\_\_

Check brakes - depress brake pedal with engine running, tractor in gear \_\_\_\_ X 10 \_\_\_\_\_

Check tires - by sight only \_\_\_\_ X 10 \_\_\_\_\_

Check hazards - dirt, grease, tools, improper attachments, etc \_\_\_\_ X 10 \_\_\_\_\_

Check safety belts \_\_\_\_ X 10 \_\_\_\_\_

Check ROPS \_\_\_\_ X 25 \_\_\_\_\_

**STARTING**

Transmission not in Neutral/ Park \_\_\_\_ X 25 \_\_\_\_\_

Brakes not set \_\_\_\_ X 25 \_\_\_\_\_

Clutch not disengaged \_\_\_\_ X 15 \_\_\_\_\_

Check Throttle Setting \_\_\_\_ X 15 \_\_\_\_\_

Check Disengagement of PTO \_\_\_\_ X 15 \_\_\_\_\_

 **TOTAL**  \_\_\_\_\_

**Score Sheet #2 – Two Wheeled Manure Spreader Event**

Contestant \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

School\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Region\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Participant is dressed appropriately for this CDE and is wearing work boots. (If box is not checked prior to the event starting, then the student may not participate on the driving course)**

**OBSTACLE COURSE Faults Points**

For touching line, stake, or twine \_\_\_\_ X 50 \_\_\_\_\_

For each time tractor or manure spreader knocks down a stake \_\_\_\_ X 100 \_\_\_\_\_

For each unnecessary change of direction (forward or backward) \_\_\_\_ X 50 \_\_\_\_\_

For Fouling Equipment (touching spreader with tractor wheel) \_\_\_\_ X 200 \_\_\_\_\_

For need to move fence/stake to allow entrance or exit of equipment \_\_\_\_ X 300 \_\_\_\_\_

**BACKING SPREADER INTO STALL**

For each 1" over 2" from rear center stake \_\_\_\_ X 15 \_\_\_\_\_

For each 1" off-center of stall

 Front Corners \_\_\_\_ X 10 \_\_\_\_\_

 Back Corners \_\_\_\_ X 10 \_\_\_\_\_

For touching line, stake, or twine \_\_\_\_ X 50 \_\_\_\_\_

For each time tractor or manure spreader knocks down a stake \_\_\_\_ X 100 \_\_\_\_\_

For Fouling Equipment (touching spreader with tractor wheel) \_\_\_\_ X 200 \_\_\_\_\_

For each unnecessary change of direction (forward or backward) \_\_\_\_ X 50 \_\_\_\_\_

Not placing manure spreader into stall after 3 attempts \_\_\_\_ X 600 \_\_\_\_\_

**JUDGES OBSERVE SAFETY AT ALL TIMES DURING ABOVE OPERATIONS**

Improper mount (on) / dismount (off) tractor \_\_\_\_ X 50 \_\_\_\_\_

Failure to use seat belt \_\_\_\_ X 25 \_\_\_\_\_

Failure to set brakes when getting off/or put in Park \_\_\_\_ X 50 \_\_\_\_\_

Sliding or spinning tires, brake steering \_\_\_\_ X 100 \_\_\_\_\_

Rough clutch engagement \_\_\_\_ X 25 \_\_\_\_\_

Clashing of gears when shifting \_\_\_\_ X 25 \_\_\_\_\_

Excessive engine speed \_\_\_\_ X 25 \_\_\_\_\_

Excessive tractor speed \_\_\_\_ X 50 \_\_\_\_\_

Excessively slow tractor speed \_\_\_\_ X 25 \_\_\_\_\_

Standing while tractor is moving \_\_\_\_ X 100 \_\_\_\_\_

Moving tractor with brakes on \_\_\_\_ X 25 \_\_\_\_\_

Failure to put in gear or park when getting off with engine stopped \_\_\_\_ X 50 \_\_\_\_\_

Any unsafe conduct while on or around tractor \_\_\_\_ X 25 \_\_\_\_\_

Riding Clutch \_\_\_\_ X 75 \_\_\_\_\_

Turning the tractor tires while not moving forward or backward \_\_\_\_ X 75 \_\_\_\_\_

 **TOTAL \_\_\_\_\_\_\_\_\_**

**Score Sheet #3 - Four Wheeled Wagon Event**

Contestant \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

School\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Region\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Participant is dressed appropriately for this CDE and is wearing work boots. (If box is not checked prior to the event starting, then the student may not participate on the driving course)**

**STARTING (verbal response to Judges) Faults Points**

Transmission not in Neutral/ Park \_\_\_\_ X 25 \_\_\_\_\_

Brakes not set \_\_\_\_ X 25 \_\_\_\_\_

Clutch not disengaged \_\_\_\_ X 15 \_\_\_\_\_

Check Throttle Setting \_\_\_\_ X 15 \_\_\_\_\_

Check Disengagement of PTO \_\_\_\_ X 15 \_\_\_\_\_

**HITCHING TRACTOR TO FOUR WHEEL WAGON**

Failure to put transmission in neutral or park \_\_\_\_ X 50 \_\_\_\_\_

Failure to set brakes \_\_\_\_ X 50 \_\_\_\_\_

For each 1” over 1” the wagon is moved (forward or backward) \_\_\_\_ X 25 \_\_\_\_\_

**WAGON HANDLING**

For touching line, stake, or twine \_\_\_\_ X 50 \_\_\_\_\_

For each time tractor or wagon knocks down a stake \_\_\_\_ X 100 \_\_\_\_\_

For each unnecessary change of direction (forward or backward) \_\_\_\_ X 50 \_\_\_\_\_

For Fouling Equipment (touching wagon tongue with tractor tire, \_\_\_\_ X 200 \_\_\_\_\_

 sliding wagon wheels sideways)

Each time any part of front wagon axle crosses 40' end line \_\_\_\_ X 400 \_\_\_\_\_

For need to move fence/stake to allow entrance or exit of equipment \_\_\_\_ X 300 \_\_\_\_\_

**WAGON PLACEMENT IN STALL**

For each 1” off center at the front of wagon \_\_\_\_ X 10 \_\_\_\_\_

For each 1” off center at the rear of wagon \_\_\_\_ X 10 \_\_\_\_\_

For each 1" over 2" from rear center stake of stall (Measure total \_\_\_\_ X 10 \_\_\_\_\_

 inches over 2” from stake to back of wagon if

 wagon is not placed into stall)

Not Placing wagon into stall after 3 Attempts (Front wagon axle must be inside

 Of the front of the wagon stall) \_\_\_\_ X 600 \_\_\_\_\_

**JUDGES OBSERVE SAFETY AT ALL TIMES DURING ABOVE OPERATIONS**

Improper mount (on) / dismount (off) tractor \_\_\_\_ X 50 \_\_\_\_\_

Failure to use seat belt \_\_\_\_ X 25 \_\_\_\_\_

Failure to set brakes when getting off/or put in Park \_\_\_\_ X 50 \_\_\_\_\_

Sliding or spinning tires, brake steering \_\_\_\_ X 100 \_\_\_\_\_

Rough clutch engagement \_\_\_\_ X 25 \_\_\_\_\_

Clashing of gears when shifting \_\_\_\_ X 25 \_\_\_\_\_

Excessive engine speed \_\_\_\_ X 25 \_\_\_\_\_

Excessive tractor speed \_\_\_\_ X 50 \_\_\_\_\_

Excessively slow tractor speed \_\_\_\_ X 25 \_\_\_\_\_

Standing while tractor is moving \_\_\_\_ X 100 \_\_\_\_\_

Moving tractor with brakes on \_\_\_\_ X 25 \_\_\_\_\_

Failure to put in gear or park when getting off with engine stopped \_\_\_\_ X 50 \_\_\_\_\_

Riding the clutch \_\_\_\_ X 25 \_\_\_\_\_

Any unsafe conduct while on or around tractor \_\_\_\_ X 25 \_\_\_\_\_

Turning the tractor tires while not moving forward or backward \_\_\_\_ X 75 \_\_\_\_\_

 **TOTAL \_\_\_\_\_\_\_\_\_\_\_\_**